EXPLOSION ALERT: SCUBA TANKS  
They explode at less then 3,000 psi/200 bar.

Please check all your tanks. If they were made by Luxfer and they are older then 06/88 (first hydro test) empty them IMMEDIATELY.

Aluminum alloy 6351 use from 1975 to 1988) may explode with no notice at operating pressure, if you do not test tank tread every year with Eddy Current tool for sustained-load crack

It happen to me yesterday while filling tanks. No one injured.

More to come on future messages.

Share this message with as many friends as possible.

ALL CYLINDERS WITH ORIGINAL HYDRO OLDER THEN 1990 WITH NOT "VE" STAMP AFTER ALL HYDRO DATES COULD EXPLODE ANY TIME AND KILL YOU OR YOUR CUSTOMERS.

WHY NOT SIMPLY CONDEMN THEM TODAY. THEY MADE THEIR TIME AND THEIR MONEY $5/YEAR..

PLEASE SHARE WITH EVERYONE YOU KNOW WHO OWN SCUBA TANKS.

SEE ATTACHED TC/DOT REQUIREMENTS

RICHARD